
**How to install Baofeng Programming Cable Driver?**

1. Get into “Window Setting”, search “Device Manager”
2. Open “Device Manager”, and unfold Port (COM & LPT) to check the existing port.
3. Connect your radio to computer via cable, check if there is new devices installed. If nothing happen, try to unplug and plug your cable in to the computer again.




4. For this step, there are two situations:

(1) If the new device do not come with an exclamation symbol, it means the driver installed successfully. Then you can start to download corresponding programming software to program you radio.

(2) If so, that means the driver goes wrong. In this case, please follow the step below to fix the issue.

A. Firstly, open the “Cable Driver.exe” which you can find it in the file. (Named “340USB” in the disc) 

B. Click “INSTALL”.



C. Try to unplug and plug your cable to the computer.

D. Open “Device Manager”, unfold Port (COM & LPT) to check the new installed port, if there is no exclamation symbol that means the cable driver runs well.

